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	Sterilizer Selection: Core Requirements Confirmation Form

	No.
	Core Selection Factors
	Customer Input / Check
	Remarks

	1
	Required Chamber Volume
	______ L
(Ref: 150 / 250 / 360 / 600 / 800 / 1000 or above)
	

	2
	Loading Method
	□ Sterilization grids only (for smaller volumes)
□ Sterilization carts + transfer carts (for 600L and above)
	

	3
	Door Configuration
	□ Single door (Type D)
□ Double door with interlock (Type S)
	

	4
	Chamber Material
	□ 304 Stainless Steel (Standard)
□ 316L Stainless Steel (Pharma/High corrosion)
	

	5
	Utilities
(Determines site modifications)
	Steam: □ External steam available (Pressure: ______ MPa) □ None
Power: □ AC380V/50Hz 3-Phase 5-Wire □ None
Air: □ 0.4~0.7MPa compressed air □ None
	

	6
	Data & Compliance
(Determines software cost)
	□ Standard (3-level authority + built-in printer)
□ Strict (FDA 21 CFR Part 11 audit trail / Data export to SCADA)
	

	7
	Load Characteristics
	Do you need to sterilize liquids (e.g., culture media)? □ Yes □ No
	

	8
	Site Access Restrictions
	Doorway size for equipment entry: Width ______ mm × Height ______ mm
	


[bookmark: _GoBack]Note to Customer:
If you are unsure about the specific parameters in Item 5 (Utilities) or Item 8 (Site dimensions), you can leave them blank. We can provide a preliminary proposal based on standard configurations first.
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